# Static Call Graph - [mini7_V2\mini7_V2.axf]

# Static Call Graph for image mini7_V2\mini7_V2.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Mon Jun 15 09:41:43 2026

### Maximum Stack Usage = 160 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ MX_TIM1_Init ⇒ HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- NMI_Handler ⇒ NMI_Handler
- UART_EndRxTransfer ⇒ UART_EndRxTransfer
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - ADC3_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - BusFault_Handler from stm32f1xx_it.o(i.BusFault_Handler) referenced from startup_stm32f103xe.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA1_Channel4_IRQHandler from stm32f1xx_it.o(i.DMA1_Channel4_IRQHandler) referenced from startup_stm32f103xe.o(RESET)
  - DMA1_Channel5_IRQHandler from stm32f1xx_it.o(i.DMA1_Channel5_IRQHandler) referenced from startup_stm32f103xe.o(RESET)
  - DMA1_Channel6_IRQHandler from stm32f1xx_it.o(i.DMA1_Channel6_IRQHandler) referenced from startup_stm32f103xe.o(RESET)
  - DMA1_Channel7_IRQHandler from stm32f1xx_it.o(i.DMA1_Channel7_IRQHandler) referenced from startup_stm32f103xe.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - DMA2_Channel3_IRQHandler from stm32f1xx_it.o(i.DMA2_Channel3_IRQHandler) referenced from startup_stm32f103xe.o(RESET)
  - DMA2_Channel4_5_IRQHandler from stm32f1xx_it.o(i.DMA2_Channel4_5_IRQHandler) referenced from startup_stm32f103xe.o(RESET)
  - DebugMon_Handler from stm32f1xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f103xe.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - FLASH_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - FSMC_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - HardFault_Handler from stm32f1xx_it.o(i.HardFault_Handler) referenced from startup_stm32f103xe.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - MemManage_Handler from stm32f1xx_it.o(i.MemManage_Handler) referenced from startup_stm32f103xe.o(RESET)
  - NMI_Handler from stm32f1xx_it.o(i.NMI_Handler) referenced from startup_stm32f103xe.o(RESET)
  - PVD_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - PendSV_Handler from stm32f1xx_it.o(i.PendSV_Handler) referenced from startup_stm32f103xe.o(RESET)
  - RCC_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - RTC_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - Reset_Handler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - SDIO_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - SPI1_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - SPI2_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - SPI3_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - SVC_Handler from stm32f1xx_it.o(i.SVC_Handler) referenced from startup_stm32f103xe.o(RESET)
  - SysTick_Handler from stm32f1xx_it.o(i.SysTick_Handler) referenced from startup_stm32f103xe.o(RESET)
  - SystemInit from system_stm32f1xx.o(i.SystemInit) referenced from startup_stm32f103xe.o(.text)
  - TAMPER_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM2_IRQHandler from stm32f1xx_it.o(i.TIM2_IRQHandler) referenced from startup_stm32f103xe.o(RESET)
  - TIM3_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM4_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM5_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM6_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM7_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - UART4_IRQHandler from stm32f1xx_it.o(i.UART4_IRQHandler) referenced from startup_stm32f103xe.o(RESET)
  - UART5_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - UART_DMAAbortOnError from stm32f1xx_hal_uart.o(i.UART_DMAAbortOnError) referenced from stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler)
  - USART1_IRQHandler from stm32f1xx_it.o(i.USART1_IRQHandler) referenced from startup_stm32f103xe.o(RESET)
  - USART2_IRQHandler from stm32f1xx_it.o(i.USART2_IRQHandler) referenced from startup_stm32f103xe.o(RESET)
  - USART3_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - UsageFault_Handler from stm32f1xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f103xe.o(RESET)
  - WWDG_IRQHandler from startup_stm32f103xe.o(.text) referenced from startup_stm32f103xe.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f103xe.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ MX_TIM1_Init ⇒ HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f103xe.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 4 bytes, rt_memclr_w.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_memclr4
  [Called By]
  - >> MX_TIM3_Init
  - >> MX_TIM1_Init
  - >> SystemClock_Config

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  __rt_memclr_w (Thumb, 78 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  _memset_w (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr_w.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  ADC_ConversionStop_Disable (Thumb, 86 bytes, Stack size 16 bytes, stm32f1xx_hal_adc.o(i.ADC_ConversionStop_Disable))
  [Stack]

  - Max Depth = 16
  - Call Chain = ADC_ConversionStop_Disable
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_ADC_Init

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DMA1_Channel4_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = DMA1_Channel4_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DMA1_Channel5_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = DMA1_Channel5_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DMA1_Channel6_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = DMA1_Channel6_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DMA1_Channel7_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = DMA1_Channel7_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DMA2_Channel3_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = DMA2_Channel3_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DMA2_Channel4_5_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = DMA2_Channel4_5_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  Error_Handler (Thumb, 4 bytes, Stack size 0 bytes, main.o(i.Error_Handler))
  [Called By]

  - >> HAL_UART_MspInit
  - >> MX_USART2_UART_Init
  - >> MX_USART1_UART_Init
  - >> MX_UART4_Init
  - >> MX_TIM3_Init
  - >> MX_TIM2_Init
  - >> MX_TIM1_Init
  - >> MX_I2C2_Init
  - >> MX_I2C1_Init
  - >> MX_ADC1_Init

  HAL_ADC_ConfigChannel (Thumb, 240 bytes, Stack size 24 bytes, stm32f1xx_hal_adc.o(i.HAL_ADC_ConfigChannel))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_ADC_ConfigChannel
  [Called By]
  - >> MX_ADC1_Init

  HAL_ADC_Init (Thumb, 272 bytes, Stack size 24 bytes, stm32f1xx_hal_adc.o(i.HAL_ADC_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_ADC_Init ⇒ HAL_ADC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_ADC_MspInit
  - >> ADC_ConversionStop_Disable
  [Called By]
  - >> MX_ADC1_Init

  HAL_ADC_MspInit (Thumb, 76 bytes, Stack size 24 bytes, adc.o(i.HAL_ADC_MspInit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_ADC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_ADC_Init

  HAL_DMA_Abort (Thumb, 70 bytes, Stack size 8 bytes, stm32f1xx_hal_dma.o(i.HAL_DMA_Abort))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_DMA_Abort
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_DMA_Abort_IT (Thumb, 296 bytes, Stack size 40 bytes, stm32f1xx_hal_dma.o(i.HAL_DMA_Abort_IT))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_DMA_Abort_IT
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_DMA_IRQHandler (Thumb, 552 bytes, Stack size 40 bytes, stm32f1xx_hal_dma.o(i.HAL_DMA_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_DMA_IRQHandler
  [Called By]
  - >> DMA2_Channel4_5_IRQHandler
  - >> DMA2_Channel3_IRQHandler
  - >> DMA1_Channel7_IRQHandler
  - >> DMA1_Channel6_IRQHandler
  - >> DMA1_Channel5_IRQHandler
  - >> DMA1_Channel4_IRQHandler

  HAL_DMA_Init (Thumb, 112 bytes, Stack size 12 bytes, stm32f1xx_hal_dma.o(i.HAL_DMA_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_DMA_Init
  [Called By]
  - >> HAL_UART_MspInit

  HAL_GPIO_Init (Thumb, 462 bytes, Stack size 40 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_MspInit
  - >> HAL_TIM_MspPostInit
  - >> HAL_I2C_MspInit
  - >> HAL_ADC_MspInit
  - >> MX_GPIO_Init

  HAL_GPIO_WritePin (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> MX_GPIO_Init

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> ADC_ConversionStop_Disable

  HAL_I2C_Init (Thumb, 376 bytes, Stack size 16 bytes, stm32f1xx_hal_i2c.o(i.HAL_I2C_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_I2C_Init ⇒ HAL_I2C_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_I2C_MspInit
  - >> HAL_RCC_GetPCLK1Freq
  [Called By]
  - >> MX_I2C2_Init
  - >> MX_I2C1_Init

  HAL_I2C_MspInit (Thumb, 134 bytes, Stack size 32 bytes, i2c.o(i.HAL_I2C_MspInit))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_I2C_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_I2C_Init

  HAL_IncTick (Thumb, 12 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 32 bytes, Stack size 8 bytes, stm32f1xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_MspInit
  - >> HAL_InitTick
  - >> HAL_NVIC_SetPriorityGrouping
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 54 bytes, Stack size 16 bytes, stm32f1xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 52 bytes, Stack size 8 bytes, stm32f1xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_MspInit
  [Called By]
  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 26 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> HAL_UART_MspInit
  - >> HAL_TIM_Base_MspInit
  - >> MX_DMA_Init

  HAL_NVIC_SetPriority (Thumb, 60 bytes, Stack size 16 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> __NVIC_SetPriority
  [Called By]
  - >> HAL_UART_MspInit
  - >> HAL_TIM_Base_MspInit
  - >> MX_DMA_Init
  - >> HAL_InitTick

  HAL_NVIC_SetPriorityGrouping (Thumb, 26 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init

  HAL_RCCEx_PeriphCLKConfig (Thumb, 224 bytes, Stack size 32 bytes, stm32f1xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_RCCEx_PeriphCLKConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_ClockConfig (Thumb, 280 bytes, Stack size 32 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_InitTick
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetPCLK1Freq (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Called By]

  - >> HAL_I2C_Init
  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Called By]

  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 58 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Called By]

  - >> HAL_RCC_ClockConfig

  HAL_RCC_OscConfig (Thumb, 778 bytes, Stack size 40 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SYSTICK_Config (Thumb, 40 bytes, Stack size 8 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> __NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick

  HAL_TIMEx_BreakCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_BreakCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_CommutCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_CommutCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_ConfigBreakDeadTime (Thumb, 84 bytes, Stack size 8 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_ConfigBreakDeadTime))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_TIMEx_ConfigBreakDeadTime
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIMEx_MasterConfigSynchronization (Thumb, 104 bytes, Stack size 16 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_MasterConfigSynchronization))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> MX_TIM3_Init
  - >> MX_TIM2_Init
  - >> MX_TIM1_Init

  HAL_TIM_Base_Init (Thumb, 90 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_Base_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_TIM_Base_Init ⇒ HAL_TIM_Base_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_TIM_Base_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> MX_TIM3_Init
  - >> MX_TIM2_Init
  - >> MX_TIM1_Init

  HAL_TIM_Base_MspInit (Thumb, 94 bytes, Stack size 8 bytes, tim.o(i.HAL_TIM_Base_MspInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_TIM_Base_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  [Called By]
  - >> HAL_TIM_Base_Init

  HAL_TIM_ConfigClockSource (Thumb, 220 bytes, Stack size 16 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_ConfigClockSource))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_TIM_ConfigClockSource ⇒ TIM_ETR_SetConfig
  [Calls]
  - >> TIM_ETR_SetConfig
  - >> TIM_TI2_ConfigInputStage
  - >> TIM_TI1_ConfigInputStage
  - >> TIM_ITRx_SetConfig
  [Called By]
  - >> MX_TIM3_Init
  - >> MX_TIM2_Init
  - >> MX_TIM1_Init

  HAL_TIM_IC_CaptureCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_IC_CaptureCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_IRQHandler (Thumb, 304 bytes, Stack size 24 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_TIM_IRQHandler
  [Calls]
  - >> HAL_TIM_TriggerCallback
  - >> HAL_TIM_PeriodElapsedCallback
  - >> HAL_TIM_PWM_PulseFinishedCallback
  - >> HAL_TIM_OC_DelayElapsedCallback
  - >> HAL_TIM_IC_CaptureCallback
  - >> HAL_TIMEx_CommutCallback
  - >> HAL_TIMEx_BreakCallback
  [Called By]
  - >> TIM2_IRQHandler

  HAL_TIM_MspPostInit (Thumb, 120 bytes, Stack size 24 bytes, tim.o(i.HAL_TIM_MspPostInit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> MX_TIM3_Init
  - >> MX_TIM1_Init

  HAL_TIM_OC_ConfigChannel (Thumb, 82 bytes, Stack size 16 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_OC_ConfigChannel))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_TIM_OC_ConfigChannel ⇒ TIM_OC2_SetConfig
  [Calls]
  - >> TIM_OC2_SetConfig
  - >> TIM_OC4_SetConfig
  - >> TIM_OC3_SetConfig
  - >> TIM_OC1_SetConfig
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_OC_DelayElapsedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_OC_DelayElapsedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_OC_Init (Thumb, 90 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_OC_Init))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_OC_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_OC_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_OC_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_OC_MspInit))
  [Called By]

  - >> HAL_TIM_OC_Init

  HAL_TIM_PWM_ConfigChannel (Thumb, 204 bytes, Stack size 16 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_ConfigChannel))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_TIM_PWM_ConfigChannel ⇒ TIM_OC2_SetConfig
  [Calls]
  - >> TIM_OC2_SetConfig
  - >> TIM_OC4_SetConfig
  - >> TIM_OC3_SetConfig
  - >> TIM_OC1_SetConfig
  [Called By]
  - >> MX_TIM3_Init

  HAL_TIM_PWM_Init (Thumb, 90 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_Init))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_PWM_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_PWM_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> MX_TIM3_Init

  HAL_TIM_PWM_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_MspInit))
  [Called By]

  - >> HAL_TIM_PWM_Init

  HAL_TIM_PWM_PulseFinishedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_PulseFinishedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_PeriodElapsedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PeriodElapsedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_TriggerCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_TriggerCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_UARTEx_RxEventCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UARTEx_RxEventCallback))
  [Called By]

  - >> HAL_UART_IRQHandler
  - >> UART_Receive_IT

  HAL_UART_ErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_ErrorCallback))
  [Called By]

  - >> HAL_UART_IRQHandler
  - >> UART_DMAAbortOnError

  HAL_UART_IRQHandler (Thumb, 616 bytes, Stack size 24 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_UART_IRQHandler ⇒ HAL_DMA_Abort_IT
  [Calls]
  - >> HAL_DMA_Abort_IT
  - >> HAL_DMA_Abort
  - >> HAL_UART_TxCpltCallback
  - >> HAL_UART_ErrorCallback
  - >> HAL_UARTEx_RxEventCallback
  - >> UART_Receive_IT
  - >> UART_EndRxTransfer
  [Called By]
  - >> USART2_IRQHandler
  - >> USART1_IRQHandler
  - >> UART4_IRQHandler

  HAL_UART_Init (Thumb, 100 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 104
  - Call Chain = HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  [Called By]
  - >> MX_USART2_UART_Init
  - >> MX_USART1_UART_Init
  - >> MX_UART4_Init

  HAL_UART_MspInit (Thumb, 620 bytes, Stack size 48 bytes, usart.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_DMA_Init
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  - >> Error_Handler
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_RxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_RxCpltCallback))
  [Called By]

  - >> UART_Receive_IT

  HAL_UART_TxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_TxCpltCallback))
  [Called By]

  - >> HAL_UART_IRQHandler

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  MX_ADC1_Init (Thumb, 70 bytes, Stack size 24 bytes, adc.o(i.MX_ADC1_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = MX_ADC1_Init ⇒ HAL_ADC_Init ⇒ HAL_ADC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_ADC_Init
  - >> HAL_ADC_ConfigChannel
  - >> Error_Handler
  [Called By]
  - >> main

  MX_DMA_Init (Thumb, 136 bytes, Stack size 8 bytes, dma.o(i.MX_DMA_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = MX_DMA_Init ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  [Called By]
  - >> main

  MX_GPIO_Init (Thumb, 262 bytes, Stack size 56 bytes, gpio.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  MX_I2C1_Init (Thumb, 50 bytes, Stack size 8 bytes, i2c.o(i.MX_I2C1_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = MX_I2C1_Init ⇒ HAL_I2C_Init ⇒ HAL_I2C_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_I2C_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MX_I2C2_Init (Thumb, 50 bytes, Stack size 8 bytes, i2c.o(i.MX_I2C2_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = MX_I2C2_Init ⇒ HAL_I2C_Init ⇒ HAL_I2C_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_I2C_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MX_TIM1_Init (Thumb, 188 bytes, Stack size 96 bytes, tim.o(i.MX_TIM1_Init))
  [Stack]

  - Max Depth = 160
  - Call Chain = MX_TIM1_Init ⇒ HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_TIM_OC_Init
  - >> HAL_TIM_OC_ConfigChannel
  - >> HAL_TIM_ConfigClockSource
  - >> HAL_TIM_Base_Init
  - >> HAL_TIMEx_MasterConfigSynchronization
  - >> HAL_TIMEx_ConfigBreakDeadTime
  - >> HAL_TIM_MspPostInit
  - >> Error_Handler
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  MX_TIM2_Init (Thumb, 98 bytes, Stack size 32 bytes, tim.o(i.MX_TIM2_Init))
  [Stack]

  - Max Depth = 64
  - Call Chain = MX_TIM2_Init ⇒ HAL_TIM_Base_Init ⇒ HAL_TIM_Base_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_TIM_ConfigClockSource
  - >> HAL_TIM_Base_Init
  - >> HAL_TIMEx_MasterConfigSynchronization
  - >> Error_Handler
  [Called By]
  - >> main

  MX_TIM3_Init (Thumb, 158 bytes, Stack size 64 bytes, tim.o(i.MX_TIM3_Init))
  [Stack]

  - Max Depth = 128
  - Call Chain = MX_TIM3_Init ⇒ HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_TIM_PWM_Init
  - >> HAL_TIM_PWM_ConfigChannel
  - >> HAL_TIM_ConfigClockSource
  - >> HAL_TIM_Base_Init
  - >> HAL_TIMEx_MasterConfigSynchronization
  - >> HAL_TIM_MspPostInit
  - >> Error_Handler
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  MX_UART4_Init (Thumb, 48 bytes, Stack size 8 bytes, usart.o(i.MX_UART4_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = MX_UART4_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MX_USART1_UART_Init (Thumb, 48 bytes, Stack size 8 bytes, usart.o(i.MX_USART1_UART_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = MX_USART1_UART_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MX_USART2_UART_Init (Thumb, 48 bytes, Stack size 8 bytes, usart.o(i.MX_USART2_UART_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = MX_USART2_UART_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.NMI_Handler))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(RESET)

  SysTick_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.SysTick_Handler))
  [Calls]

  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  SystemClock_Config (Thumb, 114 bytes, Stack size 96 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 160
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  SystemInit (Thumb, 2 bytes, Stack size 0 bytes, system_stm32f1xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f103xe.o(.text)

  TIM2_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.TIM2_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = TIM2_IRQHandler ⇒ HAL_TIM_IRQHandler
  [Calls]
  - >> HAL_TIM_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  TIM_Base_SetConfig (Thumb, 134 bytes, Stack size 20 bytes, stm32f1xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_Init
  - >> HAL_TIM_OC_Init
  - >> HAL_TIM_Base_Init

  TIM_ETR_SetConfig (Thumb, 20 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_ETR_SetConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_ETR_SetConfig
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  TIM_OC2_SetConfig (Thumb, 98 bytes, Stack size 20 bytes, stm32f1xx_hal_tim.o(i.TIM_OC2_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_OC2_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel
  - >> HAL_TIM_OC_ConfigChannel

  UART4_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.UART4_IRQHandler))
  [Stack]

  - Max Depth = 64
  - Call Chain = UART4_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ HAL_DMA_Abort_IT
  [Calls]
  - >> HAL_UART_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  USART1_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 64
  - Call Chain = USART1_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ HAL_DMA_Abort_IT
  [Calls]
  - >> HAL_UART_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  USART2_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.USART2_IRQHandler))
  [Stack]

  - Max Depth = 64
  - Call Chain = USART2_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ HAL_DMA_Abort_IT
  [Calls]
  - >> HAL_UART_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xe.o(RESET)

  main (Thumb, 54 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 160
  - Call Chain = main ⇒ MX_TIM1_Init ⇒ HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> MX_USART2_UART_Init
  - >> MX_USART1_UART_Init
  - >> MX_UART4_Init
  - >> MX_TIM3_Init
  - >> MX_TIM2_Init
  - >> MX_TIM1_Init
  - >> MX_I2C2_Init
  - >> MX_I2C1_Init
  - >> MX_GPIO_Init
  - >> MX_DMA_Init
  - >> MX_ADC1_Init
  - >> HAL_Init
  - >> SystemClock_Config
  [Called By]
  - >> __rt_entry_main

  ### Local Symbols

  __NVIC_SetPriority (Thumb, 32 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.__NVIC_SetPriority))
  [Called By]

  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config

  TIM_ITRx_SetConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.TIM_ITRx_SetConfig))
  [Called By]

  - >> HAL_TIM_ConfigClockSource

  TIM_OC1_SetConfig (Thumb, 88 bytes, Stack size 20 bytes, stm32f1xx_hal_tim.o(i.TIM_OC1_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_OC1_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel
  - >> HAL_TIM_OC_ConfigChannel

  TIM_OC3_SetConfig (Thumb, 96 bytes, Stack size 20 bytes, stm32f1xx_hal_tim.o(i.TIM_OC3_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_OC3_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel
  - >> HAL_TIM_OC_ConfigChannel

  TIM_OC4_SetConfig (Thumb, 70 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC4_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC4_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel
  - >> HAL_TIM_OC_ConfigChannel

  TIM_TI1_ConfigInputStage (Thumb, 34 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_TI1_ConfigInputStage))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TI1_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  TIM_TI2_ConfigInputStage (Thumb, 36 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_TI2_ConfigInputStage))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TI2_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  UART_DMAAbortOnError (Thumb, 16 bytes, Stack size 8 bytes, stm32f1xx_hal_uart.o(i.UART_DMAAbortOnError))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_DMAAbortOnError
  [Calls]
  - >> HAL_UART_ErrorCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler)

  UART_EndRxTransfer (Thumb, 78 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.UART_EndRxTransfer))
  [Calls]

  - >> UART_EndRxTransfer
  [Called By]
  - >> HAL_UART_IRQHandler
  - >> UART_EndRxTransfer

  UART_Receive_IT (Thumb, 194 bytes, Stack size 8 bytes, stm32f1xx_hal_uart.o(i.UART_Receive_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_Receive_IT
  [Calls]
  - >> HAL_UART_RxCpltCallback
  - >> HAL_UARTEx_RxEventCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UART_SetConfig (Thumb, 178 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_SetConfig
  [Calls]
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  [Called By]
  - >> HAL_UART_Init

  ### Undefined Global Symbols